GPIO

The GPIO applet demonstrates the use of gpio pins on the G3.

The applet will display on a console when the “Toggle GPIO 0” button is pressed. That button also toggles the GPIO 0 line. This line is on the J22 connector on pin 4.

There is also a “Clear Console” button that is used to clear the screen of messages.